For 1990-2009 cars

1. Remove the 4, 4-5 clutch apply pipe bolts/screws (611) and the 2, 4-5 clutch apply pipe retainers (610) from the transmission case cover.

Important: Do not damage the 4-5 clutch apply pipe or the transmission case cover.

2. Remove the 4-5 clutch apply pipe (609).
3. Remove the forward/direct clutch housing thrust bearing race (628) from the transmission case cover.
4. Remove the 3 forward clutch housing fluid seal rings (607) from the transmission case cover.
5. Remove the 2 forward clutch accumulator cover bolts/screws (617) and the forward clutch accumulator cover (616).
6. Remove the following components from the forward clutch accumulator cover:

• | The forward clutch accumulator piston (612)

• | The forward clutch accumulator piston fluid seal ring (613)

• | The forward clutch accumulator piston spring (614)

• | The forward clutch accumulator cover seal (615)