For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. If equipped with all wheel drive (AWD), remove the transfer case. Refer to Transfer Case Assembly Replacement .
3. Disconnect the engine wiring harness electrical connector (2) from the crankshaft position (CKP) sensor.
4. Remove the crankshaft sensor bolt.
5. Remove the crankshaft sensor.

### Installation Procedure

1. Install the crankshaft position sensor.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the crankshaft position sensor bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Connect the engine wiring harness electrical connector to the CKP sensor.
4. If equipped with all AWD, install the transfer case. Refer to Transfer Case Assembly Replacement .
5. Lower the vehicle.