For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the console. Refer to Console Replacement .
2. Remove the console upper trim plate. Refer to Front Floor Upper Console Trim Plate Replacement .

1 | Console Side Trim Panel Screw (Qty: 1) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Console Side Trim Panel - Left
3 | Retainer Clip (Qty: 3)