For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rocker Panel Molding Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rocker Panel Molding Nut
3 | Rocker Panel Integral Clip (Qty: 9)
4 | Rocker Panel Molding Integral Retainer (Qty: 8) Tip Remove the rocker panel from the vehicle by prying the clips away from the vehicle. Retainers break easily, install new retainers as necessary.