For 1990-2009 cars

#### Tools Required

J 29184 Oil Seal Installer

### Removal Procedure

1. Remove the crankshaft balancer. Refer to Crankshaft Balancer Replacement.
2. Use a flat-bladed tool in order to remove the crankshaft oil seal. Use care not to damage the engine front cover or the crankshaft.

### Installation Procedure

Important: Do not lubricate the crankshaft front oil seal or the crankshaft balancer sealing surfaces.

1. Use the J 29184 or equivalent to install the crankshaft front oil seal.
2. Install the crankshaft balancer. Refer to Crankshaft Balancer Replacement .