For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
2. Remove the drive belt. Refer to Drive Belt Replacement .
3. Support the engine. Refer to Engine Support Fixture .
4. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
5. Remove three upper engine mount bracket bolts (1).
6. Loosen right upper front engine mount bracket bolt (2).
7. Remove the upper engine mount bracket nuts (1).
8. Remove the lower bracket bolts (2).
9. Remove the ABS connector clip from the frame.
10. Remove the mount (3) and the lower bracket (4) from the vehicle.
11. Remove the upper bracket bolt (1) from the bracket.
12. Remove the upper bracket.
13. Remove the engine mount (3) from the lower bracket (4).

### Installation Procedure

1. Install the engine mount (3) to the lower bracket (4).
2. Install the engine mount upper bracket and bolt (1) to the engine. Do not tighten the bolt.
3. Install the ABS connector clip to the bracket.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the lower bracket bolts (2).

Tighten
Tighten the lower bracket bolts to 50 N·m (37 lb ft).

5. Tighten the upper engine mount bracket nuts (1).

Tighten
Tighten the upper engine mount bracket nuts to 50 N·m (37 lb ft).

6. Install the upper engine mount bracket bolts (1).

Tighten
Tighten the upper engine mount bracket bolts to 50 N·m (37 lb ft).

7. Tighten the right upper engine mount bracket bolt (2).

Tighten
Tighten the right upper engine mount bracket bolt to 110 N·m (81 lb ft).

8. Lower the vehicle.
9. Remove the engine support. Refer to Engine Support Fixture .
10. Install the drive belt. Refer to Drive Belt Replacement .
11. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .