For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the left engine splash shield. Refer to Engine Splash Shield Replacement - Left Side.
3. Support the transmission with a transmission jack.

1 | Transmission Mount Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft)
2 | Transmission Mount Nut (Qty: 2) Tighten 50 N·m (37 lb ft)
3 | Transmission Mount

#### Procedure

Using the transmission jack, lift the transmission just enough to gain clearance to remove the transmission mount from between the frame bracket and the transmission mount bracket.