For 1990-2009 cars

## Driver or Passenger Seat Back Cushion Frame Replacement Fold Flat

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat. Refer to Front Seat Replacement - Bucket .

1 | Front Seat Outer Recliner Finish Cover Refer to Front Seat Back Recliner Outer Trim Panel Replacement .
2 | Front Seat Outer Adjuster Finish Cover Refer to Front Seat Cushion Outer Trim Panel Replacement .
3 | Front Seat Inner Recliner Finish Cover Refer to Front Seat Back Recliner Inner Trim Panel Replacement .
4 | Front Seat Inner Adjuster Finish Panel Refer to Front Seat Cushion Inner Trim Panel Replacement .
5 | Front Seat Back Finish Panel Refer to Driver Seat and Passenger Seat Back Cushion Finish Panel Replacement .
6 | Front Seat Head Restraint Refer to Front Seat Head Restraint Replacement .
7 | Front Seat Head Restraint Guides Tip Squeeze the bottom of the guides together and push upward to remove.
8 | Front Seat Back Cushion Cover and Pad

#### Procedure

1. Disconnect the lower J-hook retainer from the seat back trim cover.
2. Remove the seat back trim cover and pad from the seat back frame.

9 | Front Seat Back Cushion Frame Bolt (Qty: 4) Tighten 70 N·m (52 lb ft)
10 | Front Seat Back Cushion Frame