For 1990-2009 cars

The following approximate capacities are given in English and metric conversions. See Fluid and Lubricant Recommendations for more information. All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual. Recheck fluid level after filling.

Application | Specification
--- | ---
Metric | English
Cooling System | 10.0 liters | 10.6 quarts
Engine Oil with Filter

- 3.6L Engine RPO LY7

5.2 liters

5.5 quarts

Fuel Tank | 70.0 liters | 18.5 gallons
Automatic Transaxle - AF33-5

- Automatic - Drain and Refill

7.1 liters

7.5 quarts

- Automatic - Complete Overhaul

7.8 liters

8.2 quarts

- Transaxle Fluid

3.9 liters

4.1 quarts

Transfer Case - Getrag 760 | 0.8 liters | 0.85 quarts