For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat back cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.

1 | Rear Seat No. 1 Back Release Cables Tip

1. Disconnect the seat back release cables at the inner and outer recliners.
2. The cable secures into place in the seat back panel.