For 1990-2009 cars

### Removal Procedure

1. Remove the right sound insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side.
2. Disconnect the electrical connector from the blower motor.
3. Remove the blower motor screws from the HVAC module.
4. Remove the blower motor from the HVAC module.

### Installation Procedure

1. Install the blower motor to the HVAC module.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the blower motor screws to the HVAC module.

Tighten the screws to 1.5 N·m (13 lb in).

3. Connect the electrical connector to the blower motor.
4. Install the right sound insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side.