For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Remove the shift control lever knob. Refer to Transmission Control Lever Knob Replacement .
3. Remove the shift control boot. Refer to Transmission Control Lever Boot Replacement .
4. Remove the instrument panel lower brace bezel. Refer to Instrument Panel Lower Brace Bezel Replacement .
5. Disconnect the shift control cable. Refer to Shift Control Cable Replacement .
6. Disconnect the shift control electrical connector.

1 | Shift Control Nuts (Qty 4). Notice: Refer to Fastener Notice in the Preface section. Tighten Tighten the nuts to 25 N·m (18 lb ft).
2 | Shift Control