For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove side door trim panel upper extension. Refer to Upper Extension Trim Panel Replacement .
2. Remove side door handle trim bezel. Refer to Door Handle Bezel Replacement .
3. Remove side door trim panel. Refer to Front Side Door Trim Panel Replacement and Rear Side Door Trim Panel Replacement .

1 | Side Door Inside Handle Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Side Door Inside Handle Bolt Tighten 2.5 N·m (22 lb in)
3 | Side Door Inside Handle Assembly Tip Disconnect electrical connector.
4 | Side Door Locking Rod Assembly (Qty: 2) Tip Use a flat-bladed tool to disengage rods from retaining clips.