For 1990-2009 cars

Notice: Refer to Fastener Notice in the Preface section.

1. Install the studs into the right cylinder head.

Tighten
Tighten the studs to 10 N·m (89 lb in).

2. Install a NEW right exhaust manifold gasket.
3. Install the right exhaust manifold.
4. Loosely install the right exhaust manifold nuts onto the studs in the right cylinder head.
5. Loosely install the right exhaust manifold bolts into the right cylinder head.
6. Tighten the right exhaust manifold nuts and bolts.

Tighten
Tighten the right exhaust manifold nuts and bolts to 25 N·m (18 lb ft).

7. Place the right exhaust manifold heat shield in position.
8. Install the exhaust manifold heat shield bolts.

Tighten
Tighten the exhaust manifold heat shield bolts to 10 N·m (89 lb in).