For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Support the transaxle with a height adjustable transmission stand.
3. Remove the transaxle mount to frame nuts (4).
4. Remove the transaxle mount to bracket nuts (2).
5. Raise the transaxle enough to provide clearance between the frame and mount bracket (1) in order to remove the mount (3).

### Installation Procedure

1. Position the transaxle mount in place between the frame and mount bracket (1).
2. Lower the transaxle onto the mount (3).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the transaxle mount to bracket nuts (2).

Tighten
Tighten the nuts to 37 N·m (27 lb ft).

4. Remove the transaxle mount to frame nuts (4).

Tighten
Tighten the nuts to 37 N·m (27 lb ft).

5. Remove the transmission stand.
6. Lower the vehicle.