For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .
2. Remove the instrument panel cluster assembly. Refer to Instrument Cluster Replacement .
3. Remove the fasteners securing the steering column to the instrument panel assembly, and lower the column and wheel to the floor of the vehicle out of the way. Refer to Steering Column Replacement .
4. Remove the instrument panel inflatable restraint. Refer to Inflatable Restraint Instrument Panel Module Replacement .
5. Remove the radio. Refer to Radio Replacement .
6. Remove the global positioning system antenna. Refer to Global Positioning System (GPS) Antenna Replacement .
7. Unsnap the ALDL connector from the retainer.
8. Remove the instrument panel electrical center. Refer to Instrument Panel Electrical Center or Junction Block Replacement .

1 | Instrument Panel Retainer Assembly Bolt (Qty: 6) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Instrument Panel Retainer Assembly Nut (Qty: 1) Tip This nut is driven from front of car rearward. All other nuts are driven from rear of car forward. Tighten 9 N·m (80 lb in)
3 | Instrument Panel Retainer Assembly Nut (Qty: 5) Tighten 9 N·m (80 lb in)
4 | Instrument Panel Retainer Assembly

#### Procedures

1. Remove the screws securing the HVAC ducts to the retainer assembly.
2. Note the location and routing of the wiring harness and ground straps prior to removal to ensure proper reinstallation.
3. Disconnect the wiring harness and ground straps from the retainer assembly.
4. With the aid of an assistant, remove the retainer from the vehicle.