For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left side I/P lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.

1 | Inside Air Temperature Sensor Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Inside Air Temperature Sensor

#### Procedure

Disconnect electrical connector.