For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove rear corner upper garnish molding. Refer to Body Rear Corner Garnish Molding Replacement .

1 | Seat Belt Retractor Adjuster Bolt Notice: Refer to Fastener Notice in the Preface section. Tip Apply GM P/N 12345382 (Canadian P/N 10953489), Permatex® 24200 or equivalent on all restraint fasteners prior to installation. Tighten
45 N·m (33 lb ft).

2 | Seat Belt Retractor Bolt Tighten 45 N·m (33 lb ft).
3 | Seat Belt Retractor Anchor Bolt Tighten 45 N·m (33 lb ft).
4 | Seat Belt Retractor Assembly