For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the hood in order to access the wiper arm assemblies.

1 | Windshield Washer Wiper Arm Nut (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 28 N·m (21 lb ft)
2 | Windshield Washer Wiper Arm Assembly Tip

• | Position the driver side wiper blade tip at the dot in the center of the windshield in the lower portion of the blackout strip below the dot matrix at the center of the vehicle.

• | Position the passenger side wiper blade tip at the dot near the passenger side windshield pillar portion of the blackout strip below the dot matrix.