For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
2. Disconnect the engine wiring harness electrical connector (8) from the bank 2 intake camshaft position (CMP) sensor.
3. Remove the CMP sensor bolt.
4. Remove the CMP sensor.

### Installation Procedure

1. Install the CMP sensor.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CMP sensor bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Connect the engine wiring harness electrical connector (8) to the bank 2 intake CMP sensor.
4. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.