For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the Instrument Panel Lower Brace Bezel. Refer to Instrument Panel Lower Brace Bezel Replacement .

1 | Instrument Panel Accessory Trim Plate Assembly. Tip

1. Use a flat bladed plastic trim tool in order to remove the accessory trim plate from the I/P.
2. Disconnect the electrical connectors.
3. When replacing the trim plate, transfer all necessary components.

2 | Retainer Clips (Qty 4)