For 1990-2009 cars

As the vehicle speed increases, the transmission control module (TCM) receives input signals from the automatic transmission input and output speed sensors, the throttle position sensor and other vehicle sensors to determine the precise moment to command ON the normally-low pressure control solenoid 4.

### Second Clutch Applies

#### 26 Pressure Control Solenoid 4

The 26 pressure control solenoid 4 is commanded ON, allowing actuator feed limit fluid to enter the pressure control solenoid (PCS) 26 clutch fluid circuit. PCS 26 clutch fluid is then routed through orifice #32 to the 2-6 clutch regulator valve.

#### 2-6 Clutch Regulator Valve

PCS 26 clutch fluid moves the 2-6 clutch regulator valve assembly against the 2-6 clutch regulator valve spring force to allow 26 clutch/1234 clutch feed fluid to pass through the valve. The 26 clutch/1234 clutch feed fluid is routed into the 26 clutch fluid circuit where it passes through orifice #46 and then to the spring end of the 2-6 clutch regulator valve, and to the 2-6 clutch within the case cover.

#### 2-6 Clutch

The 26 clutch fluid from the 2-6 clutch regulator valve is routed through the case cover and to the 2-6 clutch piston assembly. The 26 clutch fluid pressure moves the piston against 2-6 clutch spring force to apply the 2-6 clutch plates.

#### Drive Range, Second Gear