For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front wheel and tire assembly. Refer to Tire and Wheel Removal and Installation.

1 | Stabilizer Shaft Link Ball Stud Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tip Use the proper size allen wrench to keep the stabilizer link ball stud from rotate while removing or installing the nut. Tighten
85 N·m (63 lb ft).

2 | Stabilizer Shaft Link