For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .

1 | Headlamp Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tip Access the lower outer bolt from inside the wheelhouse liner. Tighten
9 N·m (80 lb in)

2 | Headlamp Assembly

#### Procedure

Pull the headlamp forward slightly and disconnect the forward lamp harness electrical connector from the headlamp.