For 1990-2009 cars

### Removal Procedure

Caution: In order to prevent SIR deployment, personal injury, or unnecessary SIR system repairs, do not strike the door or the door pillar in the area of the side impact sensor (SIS). Turn OFF the ignition and remove the key when performing service in the area of the SIS.

1. Remove the front fender. Refer to Front Fender Replacement .
2. Mark around the hinge location with a soft marker for installation alignment purposes.
3. Support the door.
4. With the door fully latched on the striker, remove the hinge to door bolts.
5. Remove the hinge to body bolts and remove the hinges one at a time.

### Installation Procedure

1. Position the hinge to the vehicle with the marks made prior to removal.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the hinge to door bolts.

Tighten
Tighten the bolts to 31 N·m (23 lb ft).

3. Install the hinge to body bolts.

Tighten
Tighten the bolts to 31 N·m (23 lb ft).

4. Inspect the door for proper alignment. Refer to Front Side Door Adjustment .
5. Install the front fender. Refer to Front Fender Replacement .