For 1990-2009 cars

Important: Some models use a second design inverted tooth timing drive system on the secondary drive components. Refer to Camshaft Timing Drive Design Identification for more information on specific changes.

1. Ensure that the right secondary camshaft drive chain guide (1) is being installed.
2. Position the right secondary camshaft drive chain guide.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the secondary camshaft drive chain guide bolts.

Tighten
Tighten the secondary camshaft drive chain guide bolts to 23 N·m (17 lb ft).