For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

1. Remove rear door handle bezel. Refer to Door Handle Bezel Replacement.
2. Remove rear door trim panel. Refer to Rear Side Door Trim Panel Replacement.

1 | Rear Side Door Window Switch Assembly Tip

1. Disconnect electrical connector.
2. Use a flat-bladed tool to pry switch from door handle assembly.