For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove front door trim panel. Refer to Front Side Door Trim Panel Replacement .

1 | Front Side Door Trim Panel Seal Assembly Tip

1. To remove door seal, start at top left corner and pull downward.
2. When re-installing door seal, align locating tabs near top edge of both the seal and door structure.
3. Stretch door seal tight across top edge and set in place.
4. Wet-out adhesive around entire perimeter to ensure a proper seal.