For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .

Important: In the following service procedure, it is not necessary to remove the rear suspension support. Lower the support enough to remove the stabilizer bar.

2. Lower the rear suspension support. Refer to Support Replacement .

Important: Hold the ball shaft secure with a 90° bend style TORX® bit, when removing the nut.

3. Remove the stabilizer link to stabilizer shaft nut.
4. Remove the stabilizer shaft clamp bolts.
5. Remove the stabilizer shaft clamps and bushings from the stabilizer shaft.
6. Disengage the stabilizer shaft from the stabilizer link ball studs, while removing the stabilizer shaft from the vehicle.

### Installation Procedure

1. Position the stabilizer shaft in the vehicle, while positioning the links to the stabilizer bar.
2. Install the stabilizer shaft clamps and bushings to the stabilizer shaft.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the stabilizer shaft clamp bolts.

Tighten
Tighten the bolts to 70 N·m (52 lb ft).

Important: Hold the ball shaft secure with a TORX® bit, when installing the nut.

4. Install the stabilizer link to stabilizer shaft nut.

Tighten
Tighten the nut to 50 N·m (37 lb ft).

5. Install the rear suspension support. Refer to Support Replacement .
6. Lower the vehicle.