For 1990-2009 cars

#### Tools Required

EN 46104 Water Pump Pulley Holding Tool

1. Ensure that the engine front cover and water pump are clear of old gasket material.
2. Place a new water pump gasket on the water pump.
3. Place the water pump in position on the front cover.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the water pump bolts.

Tighten
Tighten the water pump bolts to 10 N·m (89 lb in).

5. Install the water pump pulley.
6. Loosely install the water pump pulley bolts.
7. Install the EN 46104 (1) onto the water pump pulley.

Tighten
Tighten the water pump pulley bolts to 10 N·m (89 lb in).