For 1990-2009 cars

### Removal Procedure

1. Remove the Upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .
2. Remove the LH air outlet duct screws from the instrument panel retainer.
3. Remove the LH air outlet duct from the instrument panel retainer.

### Installation Procedure

1. Inspect the seals, and replace if damaged, using Kent Industries adhesive backed foam tape P/N 46485 or equivalent.
2. Install the LH air outlet duct to the instrument panel retainer.
3. Install the LH air outlet duct screws to the instrument panel retainer.

Tighten
Tighten the screws to 1.5 N·m (13 lb in).

4. Install the Upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .