For 1990-2009 cars

1. Disconnect and remove the fresh air positive crankcase ventilation (PCV) hose from the left camshaft cover fitting.
2. Remove the engine coolant air bleed pipe bracket bolts from the upper intake manifold.
3. Remove the fuel injector harness connector from the engine coolant air bleed pipe bracket.
4. Remove the engine coolant air bleed pipe.
5. Disconnect and remove the dirty air PCV hose from the intake manifold and the right camshaft cover fitting.
6. Disconnect and remove the intake manifold-to-solenoid evaporative emissions (EVAP) hose from the intake manifold and from the EVAP solenoid.
7. Remove the EVAP solenoid bolt.
8. Remove the EVAP solenoid.
9. Remove the long intake manifold bolts.
10. Remove the short intake manifold bolts.
11. Remove the intake manifold assembly.
12. Remove and discard the lower intake manifold gasket.