For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

#### Preliminary Procedures

1. Use a grease pencil to outline the upper hood hinges.
2. Prop the hood and disconnect the hood strut rod. Refer to Hood Strut Replacement

1 | Upper Hood Hinge Bolts (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Hood Tip

• | Transfer any parts as needed.

• | Adjust the hood. Refer to Hood Adjustment .