For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: When performing service on or near the SIR components or the SIR wiring, the SIR system must be disabled. Refer to SIR Disabling and Enabling . Failure to observe the correct procedure could cause deployment of the SIR components, personal injury, or unnecessary SIR system repairs.

Warning: Do not strike or jolt the inflatable restraint side impact sensor (SIS). Before applying power to the SIS make sure that it is securely fastened. Failure to observe the correct installation procedures could cause SIR deployment, personal injury, or unnecessary SIR system repairs.

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the center pillar lower molding. Refer to Center Pillar Lower Garnish Molding Replacement

1 | Inflatable Restraint Side Impact Sensor Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Inflatable Restraint Side Impact Sensor Tip

1. Slide sensor into grooves in sheet metal to ensure proper seating of sensor against body.
2. Disconnect electrical connector.