For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Console Armrest Assembly Screws | 2 N·m | 18 lb in
Console Bolts | 9 N·m | 80 lb in
Console Screws | 2 N·m | 18 lb in
Drivers Knee Bolster Reinforcement Screw | 9 N·m | 80 lb in
Front Overhead Console Screw | 2 N·m | 18 lb in
Instrument Panel Center Lower Trim Panel Assembly Screws | 2 N·m | 18 lb in
Instrument Panel Compartment Screws | 2 N·m | 18 lb in
Instrument Panel Compartment Door Screws | 2 N·m | 18 lb in
Instrument Panel Compartment Latch Screws | 2 N·m | 18 lb in
Instrument Panel Inflatable Restraint Module Bolts | 9 N·m | 80 lb in
Instrument Panel Insulator/Closeout Panel- right | 2 N·m | 18 lb in
Instrument Panel Knee Bolster Screw | 2 N·m | 18 lb in
Instrument Panel Lower Trim Panel Screws | 2 N·m | 18 lb in
Instrument Panel Lower Left Trim Panel Assembly Screws | 2 N·m | 18 lb in
Instrument Panel Lower Trim Panel Assembly Screws | 2 N·m | 18 lb in
Instrument Panel Retainer Assembly Bolts | 9 N·m | 80 lb in
Instrument Panel Retainer Assembly Nuts | 9 N·m | 80 lb in
Instrument Panel Tie Bar to Body Bolts | 25 N·m | 18 lb ft
Instrument Panel Tie Bar to Body Nuts | 9 N·m | 80 lb in
Instrument Panel Tie Bar to HVAC Module Assembly Bolts | 4 N·m | 36 lb in
Instrument Panel Tie Bar to HVAC Module Assembly Nuts | 4 N·m | 36 lb in
Instrument Panel Upper Trim Panel Bolts | 3 N·m | 27 lb in
Instrument Panel Upper Trim Panel Screws | 2 N·m | 18 lb in