For 1990-2009 cars

## Rear Seat Head Restraint Guide Replacement Outer

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear seat back filler panel. Refer to Rear Seat Back Filler Panel Replacement .

1 | Rear Seat Head Restraint

#### Procedure

1. Push the button in and raise the head restraint to the full-up position.
2. Insert a small round tool into the guide hole
3. Pull up to remove the head restraint.

2 | Rear Seat Head Restraint Guides

#### Procedure

1. Disconnect the seat back cover j-channel from the seat back frame.
2. Loosen the bottom of the seat back cover enough to reach up to access the head restraint guides.
3. Squeeze the bottom of the guides together and push upward to remove.

## Rear Seat Head Restraint Guide Replacement Inner

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear seat back filler panel. Refer to Rear Seat Back Filler Panel Replacement .

1 | Rear Seat Center Head Restraint

#### Procedure

1. Push the button in and raise the head restraint to the full-up position.
2. Insert a small round tool into the guide hole
3. Pull up to remove the head restraint.

2 | Rear Seat Center Head Restraint Guides

#### Procedure

1. Disconnect the seat back cover j-channel from the seat back frame.
2. Loosen the bottom of the seat back cover enough to reach up to access the head restraint guides.
3. Squeeze the bottom of the guides together and push upward to remove.