For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement .

1 | Front Seat Back Recliner Nut (Qty: 6) Notice: Refer to Fastener Notice in the Preface section. Tighten 45 N·m (33 lb ft)
2 | Front Seat Cushion Frame Bolt (Qty: 4) Tighten 12 N·m (9 lb ft)
3 | Front Seat Cushion Frame
4 | Front Seat Adjuster Assembly

#### Procedure

1. Use a flat-bladed tool to remove the recliner cable from the seat frame.
2. When replacing the adjuster assembly with a new unit, transfer components as necessary.