SUN VISOR LOOSE/WILL NOT HOLD POSITION (INSTALL SLEEVE). Buick Electra Estate Wagon 1987

For 1990-2009 cars

# SUN VISOR LOOSE/WILL NOT HOLD POSITION (INSTALL SLEEVE)

#### MODELS AFFECTED: 1986-1988 LESABRE AND ELECTRA WAGONS (B SERIES)

Owner comments on B-car sun visors that are loose and will not hold position can be addressed by replacing the sleeve, Part Number 8740843 with a new thicker sleeve, Part Number 17927383.

1. Loosen tensioning screw and remove sunshade from support.

2. Extract clear plastic sleeve from sunshade using needle nose pliers and replace with new sleeve (black plastic), Part Number 17927383.

3. Check rod on support assembly to be sure it does not turn within the support. If rod turns, replace support assembly.

4. Reinstall sunshade and check for proper operation.

#### WARRANTY INFORMATION

Labor Operation Number: T1370 Labor Time: .3 Hours Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.