WOODGRAIN TRANSFER-WAGON TWO TYPES OF DECAL. Buick Electra Estate Wagon 1982

For 1990-2009 cars

# WOODGRAIN TRANSFER-WAGON TWO TYPES OF DECAL

IN 1982 TWO TYPES OF LIGHT OAK WOODGRAIN TRANSFERS WERE USED ON BUICK ESTATE WAGONS. EARLY PRODUCTION VEHICLES HAVE A TRANSLUCENT TRANSFER AND LATER PRODUCTION VEHICLES HAVE AN OPAQUE TRANSFER. THESE CANNOT BE INTERCHANGED IN SERVICE SINCE THE TRANSLUCENT TYPE CHANGES COLOR ACCORDING TO THE BODY COLOR. BEFORE ORDERING REPLACEMENT TRANSFERS, BE SURE TO PROPERLY IDENTIFY YOUR REQUIREMENTS USING THE V.I.N. BREAKPOINTS AND PART NUMBERS AS LISTED BELOW. THE V.I.N. BREAKPOINT AND PART NUMBERS FOR THE TRANSLUCENT LIGHT OAK TRANSFERS ARE AS FOLLOWS: START OF PRODUCTION TO 1G4AV35Y4CX136160 PART NUMBERS - 12300186 - LEFT FRONT FENDER - 12300187 - RIGHT FRONT FENDER - 12300203 - LEFT SIDE OR TAILGATE - 12300204 - RIGHT SIDE OR TAILGATE THE V.I.N. BREAKPOINT AND PART NUMBERS FOR THE OPAQUE LIGHT OAK TRANSFERS ARE AS FOLLOWS: V.I.N.: 1G4AV35Y4CX136161 TO END OF PRODUCTION. PART NUMBERS - 12309159 - LEFT FRONT FENDER - 12309160 - RIGHT FRONT FENDER - 12309161 - LEFT SIDE OR TAILGATE - 12309162 - RIGHT SIDE OR TAILGATE NO CHANGES WERE MADE TO THE COLONIAL WALNUT TRANSFERS. PARTS INFORMATION FOR THIS MATERIAL IS CORRECT.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.