POLICE PURSUIT VEHICLES SERVICE INFORMATION. Buick Electra Estate Wagon 1985

For 1990-2009 cars

# POLICE PURSUIT VEHICLES SERVICE INFORMATION

VEHICLES AFFECTED: 1985 Pontiac Parisienne, Parisienne Brougham, and Caprice Classic Vehicles Equipped With LM1

GM of Canada has recently made available a limited number of specially equipped Pontiac Parisienne, Parisienne Brougham, and Caprice Classic vehicles.

These vehicles are heavily equipped with special equipment such as the LM1 5.7L V8 engine, heavy duty suspension, brakes, transmission cooling, and generators.

All service parts and procedures currently in place for Canadian Chevrolet Police Pursuit Vehicles (5.7L engine) in the 1985 Chevrolet Parts Catalogue and 1985 Canadian Service Manual Supplement are applicable except:

1) No A.I.R. system components or catalytic converter are required

2) The emission hose harness required is P/N 52352296 (not P/N 52353044)

3) The tune-up label required is P/N 52355297 (not P/N 14100953)

4) Transmission internal wiring and pressure switch have been revised to provide clutch engagement in 4th gear only. The pressure switch required is P/N 8643710 (not P/N 8642346) and is installed into 4th signal bore per the attached diagram.

#### NOTICE: A limited number do not have rear window defogger, C49. ------- Please check vehicle records to confirm option content.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.