REFLECTION IN WINDSHIELD INSTALL INSTRUMENT BEZEL. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# REFLECTION IN WINDSHIELD INSTALL INSTRUMENT BEZEL

#### Models Affected: 1985 Electra and Park Avenue

Comments have been received of reflection during night time driving on early production cars. This may be corrected by installing a new cluster bezel P/N 25523812 which has a longer upper visor. (See illustration) Install by removing instrument panel pad then remove six 7mm screws that hold bezel in place. Install new bezel and reinstall instrument panel pad.

WARRANTY INFORMATION

Labor Operation Number T5073

Failure Code 92

Labor Hours .4

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.