TEMPERATURE CONTROL INOPERATIVE. Buick Electra/Park Avenue 1989

For 1990-2009 cars

# TEMPERATURE CONTROL INOPERATIVE

#### VEHICLES AFFECTED: 1989 LESABRES AND ELECTRA/PARK AVENUES

Vehicles equipped with C68 Electronic Touch Climate Control, rear window grid defogger C49, and electric door locks AU3, could exhibit an inadvertent default to 24 DEG C (75 DEG F) degrees temperature set after customer selection.

If this condition is encountered, it will be necessary to replace the automatic control assembly, part number 16130885 following instructions included with the control head.

VIN breakpoints for vehicles involved are as follows:

"H" Car Buick KH487903 thru KH496786

Wentzville vehicles produced between:

"C" Car Buick K1660801 thru K1665782

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.