BALANCE SHAFT BEARING FAILURE ALL MODELS W/3800. Buick Electra/Park Avenue 1988

For 1990-2009 cars

# BALANCE SHAFT BEARING FAILURE ALL MODELS W/3800

DCS NO. 88-11 GROUP NO. 6

#### TO: ALL BUICK DEALERS

ATTN: SERVICE MANAGERS BE SURE TO REVIEW THIS INFORMATION WITH YOUR SERVICE DEPARTMENT PERSONNEL

WE HAVE RECEIVED COMMENTS FROM THE FIELD THAT SOME 1988 3800 ENGINES HAVE EXPERIENCED FAILURE IN THE BALANCE SHAFT BEARINGS AND/OR DRIVING GEARS. SHOULD YOU ENCOUNTER A CONDITION REQUIRING REMOVAL OF THE BALANCE SHAFT OR PARTIAL ENGINE REPLACEMENT, CONTACT YOUR DISTRICT SERVICE MANAGER FOR ADDITIONAL INFORMATION BEFORE ATTEMPTING REPAIRS.

B. E. ORVIS, MGR. - TECHNICAL SERVICE JS/GW 12/3/87

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.