SERVICE GUILD: FUSE LABEL CORRECTION MODELS W/ANTI-LOCK. Buick Electra/Park Avenue 1989

For 1990-2009 cars

# SERVICE GUILD: FUSE LABEL CORRECTION MODELS W/ANTI-LOCK

#### SUBJECT: FUSE LABEL CORRECTION

#### VEHICLES AFFECTED: 1988-1989 C H

The original fuse label (located on the fuse block cover door) was printed in reverse (See Figure 1).

Number 8 should read "5 amp - Elect. Brake System - Contr." Number 9 should read "5 amp - Elec. Brake Syst. - Pump." See Figure 2.

Information found in the Owner's Manual and Service Manual is correct.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.