Fastener Tightening Specifications. Buick GL7 (Export) 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Washer Solvent Container Screws | 6 N·m | 53 lb in
Wiper Arm to Shaft Nut | 48 N·m | 35 lb ft
Wiper Arm to Shaft Nut - Rear | 25 N·m | 18.4 lb ft
Wiper Linkage to Wiper Motor Crank Arm Screws | 5 N·m | 44 lb in
Wiper Module to Vehicle Screws | 10 N·m | 89 lb in
Wiper Motor Cover Screws | 2 N·m | 18 lb in
Wiper Motor Crank Arm Screw | 14-17 N·m | 124-150 lb in
Wiper Motor Mounting Screws | 7 N·m | 62 lb in
Wiper Motor Mounting Screws - Rear | 5.5 N·m | 49 lb in
Wiper Motor Shaft Nut - Rear | 6 N·m | 53 lb in