Power Door Systems Connector End Views. Buick GL7 (Export) 2000

For 1990-2009 cars

Table 1: | Door Lock Switch Plate (Door Mounted, Plunger)
Table 2: | Front Door Lock Connector C1 (Ajar Indicator Switch)
Table 3: | Front Door Lock Connector C2 (Actuator)
Table 4: | Front Door Lock Cylinder Switch
Table 5: | Front Door Lock Switch
Table 6: | Front Window Regulator Motor
Table 7: | LH Door Lock Switch Plate (Pillar Mounted, Striker)
Table 8: | LF Window Switch
Table 9: | Outside Rearview Mirror (Mirror Motor Pack and Heated Defogger)
Table 10: | Outside Rearview Mirror Remote Control Switch
Table 11: | Rear Door Lock (Actuator)
Table 12: | RF Window Switch
Table 13: | RH Door Lock Switch Plate (Pillar Mounted, Striker)
Table 14: | Sliding Door Jamb Switch

#### Door Lock Switch Plate (Door Mounted, Plunger)

Connector Part Information

• | 1216-0716

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 295 | Passenger Door Lock Actuator Feed
B | TAN | 294 | Passenger Door Unlock Actuator Feed
C-H | -- | -- | Not Used

#### Front Door Lock Connector C1 (Ajar Indicator Switch)

Connector Part Information

• | 1216-2190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 159 | Key In Ignition Output (LH)
A | BLK | 750 | Ground (RH)
B | YEL | 804 | Door Ajar Indicator Lamp Output (LH)
C | YEL | 804 | Door Ajar Indicator Lamp Output (RH)
D | BLK | 750 | Ground (LH)
D | DK BLU | 49 | Driver Door Switch Signal (RH)

#### Front Door Lock Connector C2 (Actuator)

Connector Part Information

• | 1530-0027

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 294 | Door Unlock Motor Feed
B | GRY | 295 | Door Lock Motor Feed

#### Front Door Lock Cylinder Switch

Connector Part Information

• | 1212-4583

• | 4-Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/BLK | 780 | Key Cylinder Door Lock Output
B | -- | -- | Not Used
C | BLK | 750 | Ground
D | ORN/BLK | 781 | Key Cylinder Door Unlock Output

#### Front Door Lock Switch

Connector Part Information

• | 1208-9527

• | 6-Way F Metri-Pack 280 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 195 | Door Lock Switch Input Feed
B | BLK | 750 | Ground
C | GRY | 8 | Interior Lamps Dimming Input Feed
D | WHT | 194 | Door Unlock Switch Input Feed
E | BLK | 750 | Ground
F | -- | -- | Not Used

#### Front Window Regulator Motor

Connector Part Information

• | 1212-9487

• | 2-Way F Metri-Pack 280 Series Flexlock (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 164 | Power Window Up Direction Motor Feed (LH)
A | DK BLU | 666 | Power Window Up Direction Motor Feed (RH)
B | BRN | 165 | Power Window Down Direction Motor Feed (LH)
B | BRN | 667 | Power Window Down Direction Motor Feed (RH)

#### LH Door Lock Switch Plate (Pillar Mounted, Striker)

Connector Part Information

• | 1216-0716

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 295 | Passenger Door Lock Actuator Feed
B | TAN | 294 | Passenger Door Unlock Actuator Feed
C-H | -- | -- | Not Used

#### LF Window Switch

Connector Part Information

• | 1206-4998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 165 | Power Window Down Direction Motor Feed
B | LT BLU | 166 | RF Window Switch Up Direction Feed
C | -- | -- | Not Used
D | GRY | 8 | Interior Lamps Dimming Input Feed
E | DK BLU | 164 | Power Window Up Direction Motor Feed
F | TAN | 167 | RF Window Switch Down Direction Feed
G | BLK | 750 | Ground
H | BRN | 143 | Fused Input Feed

#### Outside Rearview Mirror (Mirror Motor Pack and Heated Defogger)

Connector Part Information

• | 1206-5781

• | 6-Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 81 | Power Mirror Left/Right Motor Feed (LH)
A | RED/WHT | 881 | Power Mirror Left/Right Motor Feed (RH)
B | LT GRN | 1499 | Power Mirror Select Switch Feed (Left)
B | LT BLU/WHT | 1497 | Power Mirror Select Switch Feed (Right)
C | YEL | 88 | Power Mirror Up/Down Motor Feed (LH)
C | BRN/WHT | 1498 | Power Mirror Up/Down Motor Feed (RH)
D | -- | -- | Not Used
E | ORN | 267 | Heated Mirror Feed
F | BLK | 750 | Ground

#### Outside Rearview Mirror Remote Control Switch

Connector Part Information

• | 1204-7886

• | 8-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 1498 | RH Outside Rearview Mirror Up/Down Output Feed
B | RED/WHT | 881 | RH Outside Rearview Mirror Right/Left Output Feed
C | LT BLU/WHT | 1497 | RH Outside Rearview Mirror Motor Ground Feed
D | BLK | 750 | Ground
E | ORN | 1140 | Fused Input Feed
F | WHT | 81 | LH Outside Rearview Mirror Motor Right/Left Output Feed
G | YEL | 88 | LH Outside Rearview Mirror Motor Up/Down Output Feed
H | LT GRN | 1499 | LH Outside Rearview Mirror Motor Ground Feed

#### Rear Door Lock (Actuator)

Connector Part Information

• | 1207-7900

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 295 | Door Lock Motor Feed
B | TAN | 294 | Door Unlock Motor Feed

#### RF Window Switch

Connector Part Information

• | 1206-4998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 666 | Power Window Up Direction Motor Feed
B | GRY | 8 | Interior Lamps Dimming Input Feed
C | BLK | 750 | Ground
D | TAN | 167 | RF Window Switch Down Direction Feed
E | BRN | 667 | Power Window Down Direction Motor Feed
F | BRN | 141 | Fused Input Feed
G | -- | -- | Not Used
H | LT BLU | 166 | RF Window Switch Up Direction Feed

#### RH Door Lock Switch Plate (Pillar Mounted, Striker)

Connector Part Information

• | 1216-0716

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 295 | Passenger Door Lock Actuator Feed
B | TAN | 294 | Passenger Door Unlock Actuator Feed
C-H | -- | -- | Not Used

#### Sliding Door Jamb Switch

Connector Part Information

• | 1206-5422

• | 3-Way F Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 804 | Door Ajar Indicator Lamp Output
B | ORN | 54 | Passenger Door Switch Signal
C | BLK | 750 | Ground