Front Side Door Window Weatherstrip Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the front door window. Refer to Front Side Door Window Replacement .
4. Remove the weather-strip from the door frame.

### Installation Procedure

1. Install the weather-strip to the door frame.
2. Install the front door window. Refer to Front Side Door Window Replacement .
3. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Install the front door trim panel. Refer to Door Trim Panel Replacement .