SERVICE MANUAL UPDATE-SEC. 8D1 REVISED CODE E042 DIAG. CHART. Buick Reatta 1990

For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 8D1 REVISED CODE E042 DIAG. CHART

THIS BULLETIN IS TO UPDATE THE CODE E042 DIAGNOSTIC CHART ON PAGE 8D1-53 IN SECTION 8D1 "ECM TROUBLE CODE DIAGNOSIS" FOR THE 1990 "E" CAR WITH 3800 (VIN C) ENGINE.

THE REVISED CHART ADDRESSES THE POSSIBILITY OF A FAULTY IGNITION MODULE SETTING CODE E042 BY NOT GROUNDING THE EST SIGNAL (CKT 423) DURING CRANK.

DISCLAIMER

COPYRIGHT 1990 GENERAL MOTORS CORPORATION ALL RIGHTS RESERVED

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.