For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Frame to Underbody Bolts | 191 N·m | 141 lb ft
Inlet/Outlet Hose Retainer Bolts | 6 N·m | 53 lb in
Intermediate Steering Shaft Pinch Bolt | 47 N·m | 35 lb ft
Outer Hose Retaining Clamp Nuts | 21 N·m | 15 lb ft
Power Steering Gear Hose Fittings to Pump and Steering Gear | 27 N·m | 20 lb ft
Power Steering Pump Mounting Bolts | 27 N·m | 20 lb ft
Steering Gear Mounting Bolts | 65 N·m | 48 lb ft