For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Driver/Passenger Seat Buckle-Side Belt Nut | 41 N·m | 30 lb ft
Front Driver/Passenger Seat Shoulder Belt Bolt | 41 N·m | 30 lb ft
Front Seat Shoulder Belt Guide Bolt/Screw | 41 N·m | 30 lb ft
Guide Loop Anchor Bolt | 41 N·m | 30 lb ft
Lap Retractor Anchor Bolt | 41 N·m | 30 lb ft
Lap Retractor Trim Cover Screw | 2 N·m | 18 lb in
Rear Seat Center Belt Anchor Bolt | 41 N·m | 30 lb ft
Rear Seat Outside Belt Retractor Assembly Anchor Bolt | 41 N·m | 30 lb ft
Rear Seat Outside Belt Anchor Bolt | 41 N·m | 30 lb ft